; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPE P1
TRIG T1
IDEF A 1
  SET IP0 S0
  TIME 100
  END
PDEF B
  LIMIT (IP0,OUTSIDE,-32768,10000,T1,OUTSIDE,-32768,10000)
  WAIT (IP0, T1, 10, 10, P1)
  BAVERAGE (P1, 20, 100, $BINOUT)
  END
START A, B
