; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
TRIG T1
IDEF A 1
  SET IP0 B0
  TIME 10000
  END
PDEF B
  CHANGE (IP0,T1)
  FREQUENCY (T1, 100, $BINOUT)
  END
START A, B
