; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPE P1,P2,P3,P4,P5
IDEF A 10
  SET IP0 S0
  SET IP1 S1
  SET IP2 S0
  SET IP3 S2
  SET IP4 S0
  SET IP5 S3
  SET IP6 S0
  SET IP7 S4
  SET IP8 S0
  SET IP9 S5
  TIME 50
  END
PDEF B
  HIGH (IP(0,2,4,6,8), 100, P1)
  HIGH (IP1, 100, P2)
  HIGH (IP3, 100, P3)
  HIGH (IP5, 100, P4)
  HIGH (IP7, 100, P5)
  END
