; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPE P1
IDEF ASLAVE 1
  SLAVE
  SET IP0 S0
  TIME 5
  END
PDEF BSLAVE
  SKIP (IP0, 0, 1024, 9216, P1)
  FFT (5, 10, 2, P1, $BINOUT)
  END
