; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPES P1, P2
IDEF A 2
  SET IP0 S0
  SET IP1 S1
  TIME 100
  END
PDEF B
  AVERAGE (IP0, 100, P1)
  AVERAGE (IP1, 100, P2)
  FORMAT (P1, P2)
  END
START A, B
