; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPES P1
TRIGGER T1
IDEF A 1
  SET IPIPE0 S0
  TIME 1000
  END
PDEF B
  AVERAGE (IP0, 32, P1)
  PEAK (P1, 2, T1)
  WAIT (P1, T1, 10, 10, $BINOUT)
  END
START A, B
