; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
TRIGGER T1,T2
IDEF A 1
  SET IP0 S0
  TIME 10000
  END
PDEF B
  WAIT (IP0, T2, 100, 900, $BINOUT)
  LIMIT (IP0,INSIDE,0,32767,T1,INSIDE,0,32767)
  RETRIGGER (T1, 1000, T2) 
  END
START A, B
