; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPE P1, P2 LONG
TRIG T1
IDEF A 2
  SET IP0 S0
  SET IP1 S5
  TIME 10000
  END
PDEF B
  P1 = IP0 - IP1
  LIMIT (P1, OUTSIDE, -100, 100, T1)
  TSTAMP (T1, P2)
  MERGE (P2, $BINOUT)
  END
START A, B
