; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPES P1,P2,P3
IDEF A 4
  SET IP0 S0
  SET IP1 S1
  SET IP2 S2
  TIME 250
  END
PDEF B
  AVERAGE (IP0, 10, P1)
  AVERAGE (IP1, 20, P2)
  AVERAGE (IP2, 50, P3)
  MERGEF (P1, P2, P3, $BINOUT)
  END
START A, B
