; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
TRIGGERS T1, T2
IDEF A 1
  SET IP0 S0
  TIME 100
  END
PDEF B
  LIMIT (IP0,OUTSIDE,-32768,10000,T1,OUTSIDE,-32768,10000)
  WAIT (IP0, T2, 10, 10, $BINOUT)
  MINTIME (T1, 10000, T2)
  END
START A, B
