; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPE P1, P2 LONG
TRIG T1 2
IDEF A 1
  SET IP0 B0
  TIME 100
  END
PDEF B
  CHANGE (IP0, T1)
  WAIT (IP0, T1, 0, 1, P1)
  TSTAMP (T1, P2)
  MERGE (P2, P1, $BINOUT)
  END
START A, B
