; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPE P1 LONG
TRIGGER T1 2
IDEF A 5
  SET IP0 S0
  SET IP1 S1
  SET IP2 S2
  SET IP3 S3
  SET IP4 S4
  TIME 10
  END
PDEF B
  LIMIT (IP0,INSIDE,10000,32767,T1,INSIDE,10000,32767)
  WAIT (IP(0,1,2,3,4),T1,100,400,$BINOUT)
  TSTAMP (T1, P1)
  FORMAT (P1)
  END
START A, B
