; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPE P1,P2
PDEF B
  WAVEFORM (1, 12288, 100, P1)
  P2 = P1 + 20479
  WAVEFORM (2, 32000, 10, OPIPE0, 2, P2)
  END
ODEF C 1
  SET OPIPE0 A0
  TIME 4000
  END
START B, C
