; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPES P1,P2,P3,P4
VARIABLES V1,V2,V3,V4
IDEF A 1
  SET IP0 S0
  TIME 10000
  COUNT 1000
  END
PDEF B
  RANGE (IP0, INSIDE,   1,  1000, P1)
  RANGE (IP0, INSIDE, 1001, 2000, P2)
  RANGE (IP0, INSIDE, 2001, 3000, P3)
  RANGE (IP0, INSIDE, 3001, 4000, P4)
  PCOUNT (P1, V1)
  PCOUNT (P2, V2)
  PCOUNT (P3, V3)
  PCOUNT (P4, V4)
  END
START A, B
