; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPES P1,P2,P3,P4,P5,P6,P7 LONG
IDEF A 6
  SET IPIPE0 D0 1
  SET IPIPE1 D0 10
  SET IPIPE2 D0 100
  SET IPIPE3 G 1
  SET IPIPE4 G 10
  SET IPIPE5 G 100
  TIME 1000
  END
PDEF B
  AVERAGE (IP0, 16, P1)
  AVERAGE (IP1, 16, P2)
  AVERAGE (IP2, 16, P3)
  AVERAGE (IP3, 16, P4)
  AVERAGE (IP4, 16, P5)
  AVERAGE (IP5, 16, P6)
  AUTORANGE (6,P1,P2,P3,P4,P5,P6,P7,16)
  MERGE (P7, $BINOUT)
  END
START A, B
