; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPES P0
IDEFINE A 1
  SET IPIPE0 S0
  TIME 1000
  END
PDEFINE B
  HIGH (IP0, 300, P0)
  RANGE (P0, INSIDE, 5000, 30000, $BINOUT)
  END
START A, B
