; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPES P1,P2,P3,P4,P5
PDEF A
  SINEWAVE (30000, 100, P1)
  SQUAREWAVE (30000, 100, P2)
  TRIANGLE (30000, 100, P3)
  SAWTOOTH (30000, 100, P4)
  MERGE (P1, P2, P3, P4, P5)
  DEXPAND (P5, (0,1,2,3), OPIPE0)
  END
ODEF B 1
  SET OPIPE0 B
  TIME 250
  CYCLE 1600
  END
START A, B
