; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPES P1,P2,P3 LONG,P4 LONG
PIPES P5 LONG,P6 LONG
TRIGGERS T1,T2
IDEF A 1
  SET IP0 S0
  TIME 10000
  END
PDEF B
  AVERAGE (IP0,16,P1)
  AVERAGE (IP0,16,P2)
  PEAK (P1, 0, T1)
  PEAK (P2, 1, T2)
  TSTAMP (T1, P3)
  TSTAMP (T2, P4)
  DELTA (P3, P5)
  DELTA (P4, P6)
  MERGEF (P5, P6, $BINOUT)
  END
START A, B
