; Copyright (c) 1995,  Microstar Laboratories, Inc.
; All rights reserved.

RESET
PIPE P1 LONG
TRIGGER T1
IDEF A 1
  SET IP0 S0
  TIME 500
  END
PDEF B
  LIMIT (IP0, INSIDE, 10000, 20000, T1)
  TSTAMP (T1, P1)
  MERGE (P1, $BINOUT)
  END
START A, B
